

### ASRockRack Technical Document (Aug/2020)

**Q: How to re-write the LAN MAC address?**

|  |  |
| --- | --- |
| **Preparation** | : |

1. USB drive
2. “Eeupdate” folder and copy it into USB drive




1. Boot into Built-in EFI Shell environment

**Steps:**

1. **Check all the LAN MAC address on the mainboard.**

Command: eeupdate64.efi /all /mac\_dump

*Sample:*




1. **Write the LAN(s) MAC address.**

*LAN MAC address: refer to the white sticker on the mainboard. (If there only one sticker, that is LAN1 MAC address (HEX); plus 1 will be LAN2 MAC address and so on)*

Command: eeupdate64.efi /nic={LAN#} /mac={LAN# MAC address}

*Sample:*



1. **Reboot the system after the LAN# MAC address update process finished.**

----- END -----

*Sampel of MAC sticker:*

