**How to update BCM FW**

Test environment: UEFI SHELL

Tool: 

1. Decompress the BCM tool into USB and boot into USB under UEFI shell
2. execute 01blank.nsh to clear old FW
3. execute 02fw\_225.nsh to update new FW
4. execute 04mac.nsh to update MAC
5. AC cycle then execute “bnxtmt.efi –none” to check FW ver./mac

PS. MAC address stickers is on the LAN port

