How to use vnc connect BMC

Step 1.: Download putty and install it.

Step 2. Download ultravnc and install it.

<https://uvnc.com/downloads/ultravnc.html>

Step 3. Open Shell or Windows Command Line

Windows Command: putty.exe –ssh –L anyport:localhost:5900 UserName@{BMC IP} –pw { BMC Password }

Ex: putty.exe –ssh –L 1234:localhost:5900 [admin@192.168.36.242](mailto:admin@192.168.36.242) –pw adminadmin

Linux Command: putty –ssh –v –L {anyport}:localhost:5900 –l admin {BMC IP}

Ex: putty –ssh –v –L 1234:localhost:5900 –l admin 192.168.36.242

Key in it and then will show a window ask you key-in password ( BMC Password )

Step 4. Open VNC Software like RealVnc, Ultravnc or TightVnc

You will see it.

